I've been revisiting the config settings, in addition to the four resistors there is an additional input from pin A4 which determines if the ECU has an EGR temperature sensor (not read on 95 US models).

The four ECUs listed below all have emissions equipment

The 56B30 and 56B40 are US models, the 56B70 and 56B80 are Euro models.

The 56B30 and 56B70 are 5 speed M/T and the 56B40 and 56B80 are 3-speed A/T models

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Config Settings | | | | |
| ECU | R300 | R301 | R302 | R303 |
| 56B30 | X | X | X |  |
| 56B40 | X | X |  |  |
| .56B70 | X |  | X |  |
| 56B80 | X |  |  |  |

In the E900 code;

R303 is not read?

R302 means A/T or M/T

R301 means US model or Rest of World

R300 is not read?

A4 = California config. is read twice