**IC704 - 74HC595**

**Serial Output**



|  |  |  |
| --- | --- | --- |
| **Pin** | **Signal** | **Function** |
| 15 | Q0 | PGC |
| 1 | Q1 | PTC - Heater |
| 2 | Q2 | O2SH |
| 3 | Q3 |  |
| 4 | Q4 | ACO – AC Off Control |
| 5 | Q5 |  |
| 6 | Q6 | TA3/THO – Auto throttle position |
| 7 | Q7 | TA4 – Auto throttle position |

Where is TA2 – Auto throttle position

Maps to 0F9h